
RST® circular connector, IP66/68(3 m; 2 h)/69, male, 5-pole, light blue 

System RST® MINI - Circular connector according to IEC 61535 for permanent installation with type of protection IP66/68(3 m; 2 h)/69, male with locking, 5-pole, turned contacts with screw connection, very compact housing with strain relief, field assembly, mechanical/color coding light blue.

Rated voltage: 400 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Type of protection: up to IP66/68(3 m; 2 h)/69
Rated cross-section (fine stranded): 0.25 - 2.5 mm²
Rated cross-section (solid): 0.25 - 2.5 mm²
Cable diameter: 7.1 - 13.0 mm
Housing material: PA66, V2
Sealing material: NBR
Connections per pole: 1
Marking: 5, 4, 3, 2, 1
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: RST16I5S S1 ZR1 BL
Part No.: 46.052.4553.9
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