
RST® device connector M20, IP66/68(3 m; 2 h)/69, female, 5-pole, 400 V, 16 A, black

System RST® MINI - Device connector according to IEC 61535 for permanent installation, female, 5-pole, turned contacts with screw connection, fastening screw from inside, mechanical coding light gray/black, color coding black.

Rated voltage: 400 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Type of protection: up to IP66/68(3 m; 2 h)/69
Wall thicknesses: up to 5 mm
Rated cross-section (fine stranded): 0.25 - 2.5 mm²
Rated cross-section (solid): 0.25 - 2.5 mm²
Housing material: PA66, V2
Sealing material: NBR
Connections per pole: 1
Marking: 1, 2, 3, N, PE
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: RST16I5S B1 M00 SW
Part No.: 46.051.5053.1
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