
RST® compact distribution, IP66/68(3 m; 2 h)/69, 5-pole, 1 input, 3 outputs, 400 V, 16 A, black

System RST® MINI - RST compact distribution for circular connector IP66/68(3 m; 2 h)/69 according to IEC 61535, 1 input, 3 outputs, 5-pole, ready wired, halogen-free wires with 1.5 mm², mechanical coding light gray/black, color coding black.

Rated voltage: 400 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Type of protection: IP66/68(3 m; 2 h)/69
Housing material: PA66, V2
Sealing material: NBR
Input: 1
Outputs: 3
Halogen-free: yes
Dimension: 104x162x57.2 mm

Brand: Wieland Electric GmbH 
Type: RST16I5B 3P1 F VG SW
Part No.: 46.050.0153.1
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