
RST® circular connector, IP66/68(3 m; 2 h)/69, female, 3-pole, 400 V, 16 A, leaf green

System RST® MINI - Circular connector according to IEC 61535 for permanent installation with type of protection IP66/68(3 m; 2 h)/69, female, 3-pole, turned contacts with screw connection, very compact housing with strain relief, field assembly, mechanical/color coding leaf green.

Rated voltage: 400 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Type of protection: up to IP66/68(3 m; 2 h)/69
Rated cross-section (fine stranded): 0.25 - 1.5 mm²
Rated cross-section (solid): 0.25 - 2.5 mm²
Cable diameter: 5.0 - 9.5 mm
Housing material: PA66, V2
Sealing material: NBR
Connections per pole: 1
Marking: 1, 2, PE
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: RST16I3S B1 ZR1 GN
Part No.: 46.031.4555.7
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