
RST® compact distribution, IP66/68(3 m; 2 h)/69, 3-pole, 1 input, 2 outputs, serial connection, 400 V, 16 A, leaf green

System RST® MINI - RST compact distribution for circular connector IP66/68(3 m; 2 h)/69 according to IEC 61535, 1 input, 3 outputs, 3-pole, serial connection, with mounting option on distributor mounting plate, mechanical/color coding leaf green.

Rated voltage: 400 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Type of protection: IP66/68(3 m; 2 h)/69
Housing material: PA66, V2
Sealing material: NBR
Input: 1
Outputs: 2, serial connection
Halogen-free: yes
Dimension: 55x60x29 mm

Brand: Wieland Electric GmbH 
Type: RST16I3B 2P1 F VS GN
Part No.: 46.030.1355.7
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