
RST® distribution block, IP66/68(3 m; 2 h)/69, 2-pole, 1 input, 2 outputs, 400 V, 16 A, light blue

System RST® MINI - RST distribution block for circular connector IP66/68(3 m; 2 h)/69 according to IEC 61535, 1 input, 2 outputs, 2-pole, with mounting option on distributor mounting plate, mechanical/color coding light blue.

Rated voltage: 400 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Type of protection: IP66/68(3 m; 2 h)/69
Housing material: PA66, V2
Sealing material: NBR
Input: 1
Outputs: 2
Halogen-free: yes
Dimension: 55x60x29 mm

Brand: Wieland Electric GmbH 
Type: RST16I2B 2P1 F VG BL
Part No.: 46.030.1254.9
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