
RST® multi distribution unit, IP66/68(3 m; 2 h)/69, 2-pole, 1 input, 7 outputs, 250 V, 20 A, signal brown

System RST® CLASSIC - Distribution unit for circular connector IP66/68(3 m; 2 h)/69 according to IEC 61535, distribution unit for optional mounting of up to eight M25 device connectors IP66/68(3 m; 2 h)/69, 2-pole, 1 input, 7 outputs, ready wired, halogen-free wires with 2.5 mm².

Rated voltage: 250 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Type of protection: IP66/68(3 m; 2 h)/69
Housing material: PA66, V2
Sealing material: NBR
Input: 1
Outputs: 7
Halogen-free: yes
Dimension: 104x162x96 mm

Brand: Wieland Electric GmbH 
Type: RST20I2B 7P1 F VG BR01
Part No.: 99.946.0000.7
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