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RST® connection cable IP66/68(3 m; 2 h)/69, female, free end, 5x 2.5 mm², 250/400 V, 20 A, Cca, length: 1 m, black

System RST® CLASSIC - assembled H05Z1Z1-F connection cable with protective ground IP66/68(3 m; 2 h)/69, 5-pole, 2.5 mm², fire class Cca, female RST20i5, free end (ultrasonic welded), according to IEC 61535, mechanical coding light grey/black, color coding black.

Rated voltage: 250/400 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Type of protection: IP66/68(3 m; 2 h)/69
Cable type: H05Z1Z1-F
Fire class: Cca
Cable color: black
Halogen-free: yes
Length: 1 m

Brand: Wieland Electric GmbH 
Type: RST20I5K1B 25C 10SW
Part No.: 96.453.10C3.1

