
RST® extension cable IP66/68(3 m; 2 h)/69, female, male, 3x 1.5 mm², 250 V, 16 A, B2ca, length: 2 m, black

System RST® CLASSIC - assembled H05Z1Z1-F extension cable with protective ground IP66/68(3 m; 2 h)/69, 3-pole, 1.5 mm², fire class B2ca, with locking, male RST20i3, female RST20i3, according to IEC 61535, mechanical coding light grey/black, color coding black.

Rated voltage: 250 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Type of protection: IP66/68(3 m; 2 h)/69
Cable type: H05Z1Z1-F
Fire class: B2ca
Cable color: black
Halogen-free: yes
Length: 2 m

Brand: Wieland Electric GmbH 
Type: RST20I3K1BS 15B 20SW
Part No.: 96.232.20B0.1 
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