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RST® extension cable IP66/68(3 m; 2 h)/69, female, male, 2x 2.5 mm², low voltage, length: 4 m, signal brown

System RST® CLASSIC - assembled Ölflex Classic 110 extension cable IP66/68(3 m; 2 h)/69, 2-pole, 1.5 mm², with locking, male RST20i2, female RST20i2, according to IEC 61535, mechanical/color coding signal brown.

Rated voltage: 24 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Type of protection: IP66/68(3 m; 2 h)/69
Cable type: Ölflex Classic 110
Cable color: light grey
Halogen-free: no
Length: 4 m

Brand: Wieland Electric GmbH 
Type: RST20I2K1BS 25PL 40BR01
Part No.: 96.223.4092.4

