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RST® connection cable IP66/68(3 m; 2 h)/69, female, free end, 2x 1.5 mm², low voltage, Eca, length: 7 m, signal brown

System RST® CLASSIC - assembled H05VV-F connection cable IP66/68(3 m; 2 h)/69, 2-pole, 1.5 mm², fire class Eca, female RST20i2, free end (ultrasonic welded), according to IEC 61535, mechanical/color coding signal brown.

Rated voltage: 250 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Type of protection: IP66/68(3 m; 2 h)/69
Cable type: H05VV-F
Fire class: Eca
Cable color: black
Halogen-free: no
Length: 7 m

Brand: Wieland Electric GmbH 
Type: RST20I2K1B 15PL 70BR01
Part No.: 96.222.7007.4

