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RST® connection cable IP66/68(3 m; 2 h)/69, male, free end, 2x 1.5 mm², low voltage, length: 4 m, signal brown

System RST® CLASSIC - assembled H07RN-F connection cable IP66/68(3 m; 2 h)/69, 2-pole, 1.5 mm², with locking, male RST20i2, free end (ultrasonic welded), according to IEC 61535, mechanical/color coding signal brown.

Rated voltage: 250 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Type of protection: IP66/68(3 m; 2 h)/69
Cable type: H07RN-F
Cable color: black
Halogen-free: no
Length: 4 m

Brand: Wieland Electric GmbH 
Type: RST20I2K1S 15L 40BR01
Part No.: 96.222.4038.4

