
RST® circular connector, IP66/68(3 m; 2 h)/69, splitter connector, 7-pole, 250/400 V, 20 A, turquoise 

System RST® CLASSIC - Circular connector according to IEC 61535 for permanent installation with type of protection IP66/68(3 m; 2 h)/69, female mit splitter connector (two cable glands), 7-pole, turned contacts with screw connection, compact housing with strain relief, field assembly, mechanical/color coding turquoise.

Rated voltage: 250/400 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Type of protection: up to IP66/68(3 m; 2 h)/69
Terminal cross section: 0,2 - 0.75 mm²
Cable diameter: 6.0 - 10.0 mm (H05VV, H07RN-F)
Housing material: PA66, V2
Sealing material: NBR
Connections per pole: 2
Marking: L, N, PE, 1, 2, 3, 4
Halogen free: yes

Brand: Wieland Electric GmbH 
Type: RST20I7S B1 ZRX TB04
Part No.: 96.071.4253.6
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