
RST® device connector M16, IP66/68(3 m; 2 h)/69, male, 7° angled, 5-pole, 250 V + dimming, turquoise

System RST® CLASSIC - Device connector according to IEC 61535 for permanent installation, male with locking, 5-pole, 7° angled, turned contacts with screw connection fastening screw from inside, mechanical/color coding turquoise.

Rated voltage: 250/400 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Type of protection: up to IP66/68(3 m; 2 h)/69
Thread: M16x1.5
Terminal cross-section: 0.75 - 4.0 mm²
Housing material: PA66, V2
Sealing material: NBR
Connections per pole: 1
Marking: D2, D1, N, PE, L
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: RST20I5S S1 M13A TB04
Part No.: 96.056.6153.6
[bookmark: _GoBack]

