
RST® device connector M16, IP66/68(3 m; 2 h)/69, female, 5-pole, 250 V + dimming, turquoise

System RST® CLASSIC - Device connector according to IEC 61535 for permanent installation, female, 5-pole, turned contacts with screw connection fastening screw from inside, mechanical/color coding turquoise.

Rated voltage: 250/400 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Type of protection: up to IP66/68(3 m; 2 h)/69
Thread: M16x1.5
Terminal cross-section: 0.75 - 4.0 mm²
Housing material: PA66, V2
Sealing material: NBR
Connections per pole: 1
Marking: L, PE, N, D1, D2
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: RST20I5S B1 M03A TB04
Part No.: 96.051.6153.6
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