
RST® circular connector, IP66/68(3 m; 2 h)/69, splitter connector, 3-pole, 250 V, 20 A, light grey 

System RST® CLASSIC - Circular connector according to IEC 61535 for permanent installation with type of protection IP66/68(3 m; 2 h)/69, male with splitter connector (two cable glands), 3-pole, turned contacts with screw connection, compact housing with strain relief, field assembly, mechanical coding light grey/black, color coding light grey.

Rated voltage: 250 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Type of protection: up to IP66/68(3 m; 2 h)/69
Terminal cross-section: 0.75 - 2.5 mm²
Cable diameter: 6.0 - 10.0 mm (H05VV, H07RN-F)
Housing material: PA66, V2
Sealing material: NBR
Connections per pole: 2
Marking: L, N, PE
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: RST20I3S S1 ZRX GL
Part No.: 96.032.4253.0
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