
RST® circular connector, IP66/68(3 m; 2 h)/69, female, 3-pole, switching functionality, 250 V, light blue 

System RST® CLASSIC - Circular connector according to IEC 61535 for permanent installation with type of protection IP66/68(3 m; 2 h)/69, female, 3-pole, turned contacts with screw connection, compact housing with strain relief, field assembly, mechanical/color coding light blue.

Rated voltage: 250 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Type of protection: up to IP66/68(3 m; 2 h)/69
Terminal cross-section: 0.75 - 6.0 mm²
Cable diameter: 6.0 - 10.0 mm (H05VV, H07RN-F)
Housing material: PA66, V2
Sealing material: NBR
Connections per pole: 1
Marking: 1, 2, 3
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: RST20I3S B1 ZR1S BL07
Part No.: 96.031.4053.9
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