
RST® Distribution block, IP66/68(3 m; 2 h)/69, 3-pole, 1 input, 3 outputs, with mounting option, 250 V, 20 A, black

System RST® CLASSIC - Distribution block for circular connector IP66/68(3 m; 2 h)/69 according to IEC 61535, combined distribution block, H shaped, 3-pole, turned contacts, 1 input, 3 outputs, with integrated locking, with mounting option, mechanical coding light grey/black, color coding black.

Rated voltage: 250 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Type of protection: IP66/68(3 m; 2 h)/69
Housing material: PA66, V2
Sealing material: NBR
Input: 1
Outputs: 3
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: RST20I3V 3P1 F V SW
Part No.: 96.030.0153.1
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