
RST® circular connector, IP66/68(3 m; 2 h)/69, splitter connector, 2-pole, low voltage, signal brown 

System RST® CLASSIC - Circular connector according to IEC 61535 for permanent installation with type of protection IP66/68(3 m; 2 h)/69, female with splitter connector (two cable glands), 2-pole, turned contacts with spring clamp connection, compact housing with strain relief, field assembly, mechanical/color coding signal brown.

Rated voltage: 250 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Type of protection: up to IP66/68(3 m; 2 h)/69
Terminal cross-section, solid: 0.5 - 2.5 mm²
Terminal cross-section, fine-stranded: 0.5 - 1.5 mm²
Terminal cross-section, fine-stranded: 0.75 - 1.5 mm²
Cable diameter: 6.0 - 10.0 mm (H05VV, H07RN-F)
Housing material: PA66, V2
Sealing material: NBR
Connections per pole: 2
Marking: 1, 2
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: RST20I2F B23ZRXS L BR01
Part No.: 96.021.0251.4
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