[bookmark: _GoBack]
RST® connection cable IP66/68(3 m; 2 h)/69, female, free end, 5x 2.5 mm², 250/400 V, 16 A, length: 0.5 m, black

System RST® MINI - assembled H07RN-F connection cable IP66/68(3 m; 2 h)/69, 5-pole, 2.5 mm², with locking, female RST16i5, free end (ultrasonic welded), according to IEC 61535, mechanical coding light gray/black, color coding black.

Rated voltage: 250/400 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Type of protection: IP66/68(3 m; 2 h)/69
Cable type: H07RN-F
Cable color: black
Halogen-free: no
Length: 0.5 m

Brand: Wieland Electric GmbH  
Type: RST16I5K1B 25G 05SW
Part No.: 46.453.0533.1

