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RST® connection cable IP66/68(3 m; 2 h)/69, female, free end, 3x 2.5 mm², 250 V, 16 A, Eca, length: 2 m, black

System RST® MINI - assembled H05VV-F connection cable IP66/68(3 m; 2 h)/69, 3-pole, 2.5 mm², fire class Eca, with locking, female RST16i3, free end (ultrasonic welded), according to IEC 61535, mechanical coding light gray/black, color coding black.

Rated voltage: 250 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Type of protection: IP66/68(3 m; 2 h)/69
Cable type: H05VV-F
Fire class: Eca
Cable color: black
Halogen-free: no
Length: 2 m

Brand: Wieland Electric GmbH  
Type: RST16I3K1B 25P 20SW
Part No.: 46.433.2003.1

