
podis® CON Connection module, 5G6 mm², RST20i5, IP65, 690V, 20 A, black

System podis® CON - Connection module with reduced height 5G6 RST for pluggable connection with RST20i5; 5-pole; nominal ratings acc. VDE 20 A; 690 V; nominal ratings acc. UL 20 A; 600 V; degree of protection IP65; piercing contacts; Torx 15; housing black; mounting position any; outline dimensions 217x84x59 mm (LxWxH).

Rated voltage: 690 V
Rated current: 20 A
No. of Poles: 5
Degree of protection: IP65
Cross-Section: 6 mm²
Halogen-free: yes
Color: black

Brand: Wieland Electric GmbH
Type: FCS 6 5 SI SA RST20i5 LH
Part No.: 75.252.0153.1 
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