
RST® Device connector, IP66/67/69K, female, 4-pole, 250/400 V, 50 A, fixed in position

System RST® POWER - Device connector with type of protection IP66/67/69K, female, 4-pole, turned contacts with screw connection fixed in position, compact housing with strain relief, field assembly, mechanical/color coding black.

Rated voltage: 250/400 V
Rated current: 50 A
Rated impulse voltage: 4 kV
Type of protection: up to IP66/67/69K
Terminal cross-section: 4.0 - 16.0 mm²
Cable gland: M32
Housing material: PA66, V2
Sealing material: NBR
Connections per pole: 1
Marking: PE, 1, 2, 3
Halogen-free: yes

Brand: Wieland Electric GmbH
Type: RST50I4S B1 ZM02V SW
Part No.: 97.041.5553.1
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