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gesis® connection cable, female, free end, 3x 1.5 mm², 250 V, 16 A, Eca, length: 2 m, brown/black

System gesis® MINI - assembled H05VV-F connection cable without protective ground, 3-pole, 1.5 mm², fire class Eca, female GST15i3, free end, according IEC 61535, mechanical coding code 4, color coding brown.

Rated voltage: 250 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Type of protection (plugged): IP40
Type of protection (unplugged): IP20
Cable type: H05VV-F
Fire class: Eca
Cable color: black
Halogen-free: no
Length: 2 m

Brand: Wieland Electric GmbH 
Type: GST15i3 KS B- 15 W 20SW
Part No.: 91.232.2003.4

