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gesis® connection cable, female, free end, 2x 1.5 mm², 250 V, 6 A, Eca, length: 7 m, pastel blue

System gesis® MINI - assembled H05Z1Z1-F connection cable, 2-pole, 1.5 mm², fire class Eca, for dimming applications, female GST15i2, free end, according IEC 61535, mechanical coding code 2, color coding pastel blue.

Rated voltage: 250 V
Rated current: 6 A
Rated impulse voltage: 4 kV
Type of protection (plugged): IP40
Type of protection (unplugged): IP20
Cable type: H05Z1Z1-F
Fire class: Eca
Cable color: white
Halogen-free: yes
Length: 7 m

Brand: Wieland Electric GmbH 
Type: GST15i2 KS B- 15 HW 70PB01
Part No.: 91.222.7063.9

