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gesis® connection cable, female, free end, 2x 1.5 mm², 50 V, 16 A, Eca, length: 7 m, light blue

System gesis® MINI - assembled H05VV-F connection cable, 2-pole, 1.5 mm², fire class Eca, for low voltage applications, female GST15i2, free end, according IEC 61535, mechanical coding code 2, color coding light blue.

Rated voltage: 50 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Type of protection (plugged): IP40
Type of protection (unplugged): IP20
Cable type: H05VV-F
Fire class: Eca
Cable color: white
Halogen-free: no
Length: 7 m

Brand: Wieland Electric GmbH 
Type: GST15i2 KS B- 15 W 70BL02
Part No.: 91.222.7003.6

