
gesis® IDC adapter, 3-pole, 1 input, 2 outputs, 250 V, 20 A, white

System gesis® CLASSIC - GST18i3 female cable output 3-pole with IDC connection, useable for solid and stranded wires in existing installations 1.5 - 2.5 mm², 250 V, 20 A, mechanical coding code 1, color coding white, housing color white.

Rated voltage: 250 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Terminal cross-section, solid: 1.5 - 2.5 mm²
Terminal cross-section, 7-stranded: 1.5 mm²
Type of protection: IP40
Housing material: Polyamide
Input/forwarding: standard cable e.g. NYM
Output: 3-pole female GST18i3
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: GST18i3 B2HZR1 M WS 
Part No.: 92.731.6053.0
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