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gesis® extension cable, female, male, 3x 2.5 mm², 250 V, 20 A, Eca, length: 4 m, tomato red

System gesis® CLASSIC - assembled H05Z1Z1-F extension cable with protective ground, 3-pole, 2.5 mm², fire class Eca, male GST18i3, female GST18i3, according IEC 61535, mechanical coding code 2, color coding tomato red.

Rated voltage: 250 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Type of protection: IP40
Cable type: H05Z1Z1-F
Fire class: Eca
Cable color: black
Halogen-free: yes
Length: 4 m

Brand: Wieland Electric GmbH 
Type: GST18i3 K1 BS 25H 40TR01
Part No.: 92.298.4060.0

