[bookmark: _GoBack]
gesis® extension cable, female, male, 3x 2.5 mm², 250 V, 20 A, Eca, length: 5 m, black

System gesis® CLASSIC - assembled H05VV-F extension cable with protective ground, 3-pole, 2.5 mm², fire class Eca, male GST18i3, female GST18i3, according IEC 61535, mechanical coding code 1, color coding black.

Rated voltage: 250 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Type of protection: IP40
Cable type: H05VV-F
Fire class: Eca
Cable color: black
Halogen-free: no
Length: 5 m

Brand: Wieland Electric GmbH 
Type: GST18i3 K1 BS 25E 50SW
Part No.: 92.238.5000.1

