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gesis® extension cable, female, male, 3x 1.5 mm², 250 V, 16 A, Eca, length: 5 m, white

System gesis® CLASSIC - assembled H05VV-F extension cable with protective ground, 3-pole, 1.5 mm², fire class Eca, male GST18i3, female GST18i3, according IEC 61535, mechanical coding code 1, color coding white.

Rated voltage: 250 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Type of protection: IP40
Cable type: H05VV-F
Fire class: Eca
Cable color: white
Halogen-free: no
Length: 5 m

Brand: Wieland Electric GmbH 
Type: GST18i3 K1 BS 15E 50WS
Part No.: 92.232.5000.2

