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gesis® cable, female, SCHUKO male plug, 3x 1.5 mm², 250 V, 16 A, length: 1 m, black

System gesis® CLASSIC - assembled H05VV-F cable with protective ground, 3-pole, 1.5 mm², female GST18i3 with SCHUKO male plug according to DIN 49441, mechanical coding code 1, color coding black.

Rated voltage: 250 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Type of protection: IP40
Cable type: H05VV-F
Cable color: black
Halogen-free: no
Length: 1 m

Brand: Wieland Electric GmbH 
Type: GST18i3 K1 BD 15 10SW
Part No.: 92.232.1007.1

