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gesis® extension cable, female, male, 4x 2.5 mm², 250/400 V, 20 A, Eca, length: 2 m, white

System gesis® CLASSIC - assembled H05VV-F extension cable with protective ground, 4-pole, 2.5 mm², fire class Eca, male GST18i4, female GST18i4, according IEC 61535, mechanical coding code 1, color coding white.

Rated voltage: 250/400 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Type of protection: IP40
Cable type: H05VV-F
Fire class: Eca
Cable color: white
Halogen-free: no
Length: 2 m

Brand: Wieland Electric GmbH 
Type: GST18i4 K1 BS 25E 20WS
Part No.: 92.208.2000.2

