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RST® MICRO extension cable IP66/68(3m;2h)/69, female, male, 3x 0.75 mm², 250/400 V, 6 A, length: 4 m, with contact seal, black

System RST® MICRO - assembled H05RN-F extension cable IP66/68(3m;2h)/69, 3-pole, 0.75 mm², with locking, with contact seal, male RST08i3, female RST08i3, mechanical/color coding black.

Rated voltage: 250/400 V
Rated current: 6 A
Type of protection: IP66/68(3m;2h)/69
Cable type: H05RN-F
Cable color: black
Halogen-free: no
Length: 4 m

Brand: Wieland Electric GmbH  
Type: RST08I3 BS 08P 40SW
Part No.: 4L.437.4030.1

