
RST® MICRO device connector M14, IP66/68(3m;2h)/69, male, 2-pole, 250/400 V, 8 A, with contact seal, light blue

System RST® MICRO - Device connector, male, 2-pole, turned contacts with screw connection, with contact seal, fastening screw from inside, mechanical/color coding light blue.

Rated voltage: 250/400 V
Rated current: 8 A
Rated impulse voltage: 4 kV
Type of protection: up to IP66/68(3m;2h)/69
Rated cross-section (single-stranded): 0.2 - 1.0 mm²
Rated cross-section (fine-stranded): 0.22 - 1.0 mm²
Housing material: Polyamide, halogen-free, V0, f1
Seal material: NBR
Connection per pole: 1
Marking: 1, 2/N
Halogen-free: yes

Brand: Wieland Electric GmbH
Type: RST08I2S S1 M00 BL
Part No.: 4L.022.4043.9
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