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RST® MICRO connection cable IP66/68(3m;2h)/69, male, free end, 2x 0.75 mm², ~50/-120 V, 6 A, length: 2.5 m, pebble grey

System RST® MICRO - assembled H05RN-F connection cable IP66/68(3m;2h)/69, 2-pole, 0.75 mm², with locking, male RST08i2, free end (ultrasonic welded), mechanical/color coding pebble grey.

Rated voltage: ~50/-120 V
Rated current: 6 A
Type of protection: IP66/68(3m;2h)/69
Cable type: H05RN-F
Cable color: black
Halogen-free: no
Length: 2.5 m

Brand: Wieland Electric GmbH  
Type: RST08I2 -S 08P 25GR
Part No.: 41.427.2538.8

