
RST® cable, female, CEE 7/4-male, 3x 1.5 mm², 250 V, 16 A, length: 1.5 m, black

System RST® CLASSIC - assembled H07RN-F cable with protective ground, 3-pole, 1.5 mm², female RST20i3 mit CEE 7/4-male according to DIN 49441, mechanical coding light grey/black, color coding black.

Rated voltage: 250 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Cable type: H07RN-F
Cable color: black
Halogen-free: no
Length: 1.5 m

Brand: Wieland Electric GmbH 
Type: RST20I3K1BI 15 15SW
Part No.: 99.712.0000.7
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