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RST® connection cable IP66/68(3 m; 2 h)/69, male, free end, 3x 1.5 mm², 250 V, 16 A, length: 4 m, leaf green

System RST® CLASSIC - assembled H07RN-F connection cable with protective ground IP66/68(3 m; 2 h)/69, 3-pole, 1.5 mm², with locking, male RST20i3, free end (ultrasonic welded), according to IEC 61535, mechanical/color coding leaf green.

Rated voltage: 250 V
Rated current: 16 A
Rated impulse voltage: 4 kV
Type of protection: IP66/68(3 m; 2 h)/69
Cable type: H07RN-F
Cable color: black
Halogen-free: no
Length: 4 m

Brand: Wieland Electric GmbH 
Type: RST20I3K1S 15H 40GN02
Part No.: 96.232.4036.7

