
RST® device connector M20, IP66/68(3 m; 2 h)/69, male, angled, 7-pole, 250 V, light blue

System RST® CLASSIC - Device connector according to IEC 61535 for permanent installation, male, 7-pole, angled, turned contacts with screw connection, fastening screw from inside, mechanical/color coding light blue.

Rated voltage: 250/400 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Type of protection: up to IP66/68(3 m; 2 h)/69
Thread: M20x1,5
Terminal cross section: 0.2 - 2.5 mm²
Housing material: PA66, V2
Sealing material: NBR
Connections per pole: 1
Marking: 1, 2, 3, 4/N, 5, 6, 7
Halogen free: yes

Brand: Wieland Electric GmbH 
Type: RST20I7S S1 M10A BL
Part No.: 96.074.6053.9
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