
RST® device connector M25, IP66/68(3 m; 2 h)/69, female, angled, 5-pole, switching functionality, 250 V, light blue

System RST® CLASSIC - Device connector according to IEC 61535 for permanent installation, female, 5-pole, 90° angled, turned contacts with screw connection fastening screw from inside, mechanical/color coding light blue.

Rated voltage: 250/400 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Type of protection: up to IP66/68(3 m; 2 h)/69
Thread: M25x1.5
Terminal cross-section: 0.75 - 4.0 mm²
Housing material: PA66, V2
Sealing material: NBR
Connections per pole: 1
Marking: 1, 2, 3/N, 4, 5
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: RST20I5S B1 M12 BL07
Part No.: 96.053.6253.9
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