
RST® device connector M16, IP66/68(3 m; 2 h)/69, male, 3-pole, 250 V, 20 A, light grey

System RST® CLASSIC - Device connector according to IEC 61535 for permanent installation, male with locking, 3-pole, turned contacts with screw connection fastening screw from inside, mechanical coding light grey/black, color coding light grey.

Rated voltage: 250 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Type of protection: up to IP66/68(3 m; 2 h)/69
Thread: M16x1.5
Terminal cross-section: 0.75 - 6.0 mm²
Housing material: PA66, V2
Sealing material: NBR
Connections per pole: 1
Marking: N, L, PE
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: RST20I3S S1 M03 GL
Part No.: 96.032.6153.0
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