
RST® device connector M25, IP66/68(3 m; 2 h)/69, female, 3-pole, 250 V, 20 A, black

System RST® CLASSIC - Device connector according to IEC 61535 for permanent installation, female, 3-pole, turned contacts with spring clamp connection, fastening screw from outside, mechanical coding light grey/black, color coding black.

Rated voltage: 250 V
Rated current: 20 A
Rated impulse voltage: 4 kV
Type of protection: up to IP66/68(3 m; 2 h)/69
Thread: M25x1.5
Terminal cross-section, solid: 0.5 - 2.5 mm²
Terminal cross-section, fine-stranded: 0.5 - 1.5 mm²
Terminal cross-section, fine-stranded: 0.75 - 1.5 mm²
Housing material: PA66, V2
Sealing material: NBR
Connections per pole: 2
Marking: L, N, PE
Halogen-free: yes

Brand: Wieland Electric GmbH 
Type: RST20I3F B2 M01 SW
Part No.: 96.031.1053.1
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